{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":11,"rows_kept":6,"merged":[[0,0,0,10],[2,0,2,10]]}
["材料表"]
["序号","名称","规格、型号","单位","品牌、厂家","等级","含税到场价","税点（%）","不含税到场价","电话号码","备注"]
["地面"]
[1,"无方向抗碘酊，耐酸碱同透 T级耐磨PVC地板及焊条","1.同质透心无方向碎花纹，厚度2.0mm，耐污能力EN423抗11项化学试剂，不含回收料，不含邻苯类增塑剂39项，采用环保无害DOTP非邻苯类增塑剂；\n▲2通过欧盟认证Reach197项高致害物质检测测试。通过室内空气安全认证Floorscore和Green label认证，TVOC释放量小于5ug/m3，不含甲醛及重金属，通过EN743-3可溶性重金属检测19项，（汞，镉，砷，钡，磞，铅…）；\n▲3.有害物质VOC GB18586-GB119821检测报告，氯乙烯单体可溶性重金属，铅、镉未检出；。                 \n▲4.防火：通过燃烧有害烟毒性测试BS 6853  认证。GB8624、EN13501基本防火等级B1级测试；","m2"]
[2,"抛光砖","600*600","m2"]
[3,"踢脚线","100mm高抛光砖","m2"]