{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":11,"rows_kept":10,"merged":[[0,0,0,10]]}
["材料表"]
["序号","名称","规格、型号","单位","品牌、厂家","等级","含税到场价","税点（%）","不含税到场价","电话号码","备注"]
[]
[]
[3,"50厚玻镁彩钢板天花 (手工板）（用于天棚处）","1、双面0.426mm防腐喷                2、总厚度50mm\n3、产品具有表面美观、隔音、绝热、保温、抗震，防火性能符合国家标准                         4、安装方式：采用铝合金型材加L50*4角钢，与楼板或梁固定                                                ","m2"]
[4,"彩钢板吊顶龙骨吊件（上人型）","采用铝合金型材加50*50*4角铁，固定于楼顶上（上人型）","m2"]
[5,"顶部检修口","600*600mm(并用铝合金包边，收口，门材质同天花材质）","个"]
[6,"T型铝槽","承重连接使用","m"]
[7,"50厚玻镁彩钢板隔断 (手工板）（用在墙面上）","1、双面0.426mm防腐喷                2、总厚度50mm\n3、产品具有表面美观、隔音、绝热、保温、抗震，防火性能符合国家标准                         4、安装方式：采用铝合金型材加L50*4角钢，与楼板或梁固定                                                ","m2"]
[8,"铝合金型材（固定玻镁板）","1.50U型地槽，50U型天槽，50外圆形立柱，50内圆弧净化铝材                                         2.厚度1mm，6米长\n3.产品具有表面电泳防腐处理                       4.安装方式：铝合金底座卡结式                           ","m2"]