{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"merged":[[0,0,0,10],[2,0,2,10]]}
["材料表"]
["序号","名称","规格、型号","单位","品牌、厂家","等级","含税到场价","税点（%）","不含税到场价","电话号码","备注"]
["门窗"]
[1,"50MM双层密封中空窗1180*1000（带除湿，黑色丝印边）","1、50MM厚.成品定制\n2、40高强度铝合金材质内框 　      　   3、双层5厚钢化玻璃                        4、密封处理，与外界空气隔离，                               5、带除湿黑色丝印边                ","樘"]
[2,"50MM双层密封中空窗1500*1000（带除湿，黑色丝印边）","1、50MM厚.成品定制\n2、40高强度铝合金材质内框 　      　   3、双层5厚钢化玻璃                        4、密封处理，与外界空气隔离，                               5、带除湿黑色丝印边                ","樘"]
[3,"50MM双层密封中空窗1800*1000（带除湿，黑色丝印边）","1、50MM厚.成品定制\n2、40高强度铝合金材质内框 　      　   3、双层5厚钢化玻璃                        4、密封处理，与外界空气隔离，                               5、带除湿黑色丝印边                ","樘"]
[4,"钢化玻璃采集窗","12厚钢化玻璃，底部留洞口，四周磨边处理，限位凹槽，底部安装橡胶垫块，玻璃周边封密封胶\n尺寸：1.55m*2.1m","m2"]
[5,"成品洁净密闭单开门(带真空玻璃视窗）","1、饰面板材质：0.6mm鞍钢的彩钢板；           \n2、门体包边与门框为6063-T5铝合金材质，门框表面处理为：氧化；             \n3、规格尺寸：950*2100总厚度50mm；\n4、配分体锁，带窗450*650；                   5、芯材：铝蜂窝；                             6、含升降扫地条。","樘"]
[6,"成品洁净密闭子母门(带真空玻璃视窗）","1、饰面板材质：0.6mm鞍钢的彩钢板；           \n2、门体包边与门框为6063-T5铝合金材质，门框表面处理为：氧化；             \n3、规格尺寸：1350*2100总厚度50mm；\n4、配分体锁，带窗450*650；                   5、芯材：铝蜂窝；                             6、含升降扫地条。","樘"]
[7,"门禁系统","含门禁控制器、门禁电源箱、磁力锁、闭门器，出门开关、门禁读卡器、IC卡、电线","套"]
[8,"自动闭门器",null,"套"]
[9,"双门机械互锁",null,"套"]
[10,"玻璃采集窗上水晶字","150高，有机玻璃字底，亚克力字面","个"]
[11,"大理石窗台","20厚黑金砂石材，磨边处理","m2"]
[12,"自净式304不锈钢洁净传递窗","（1）自净式；　　　　　　　　　　　　　　　　　　　　　　　　（2）304不锈钢，厚1.0mm 　　　　　　　　　　　　（3）配置一支10WX1紫外线杀菌灯　 　　　　　　　　　　　　　　　 （4）双门互为连锁，设有电子或机械连锁装置；                      　　　　　　　　　　　　　　　　                                                   （5）600*600*600","套"]
[13,"不锈钢包窗套","15厘阻燃夹板底，1.0厚304不锈钢材质","m2"]
[14,"不锈钢包门套","15厘阻燃夹板底，1.0厚304不锈钢材质","m2"]